# Anik F2 @ 111.1W C-BAND
# freq pol sr fec

[CHANNEL]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 4104000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 4143000
	INNER_FEC = 1/2
	MODULATION = QPSK
	INVERSION = AUTO

