inherit kernel-uboot kernel-artifact-names uboot-sign

KERNEL_IMAGETYPE_REPLACEMENT = ""

python __anonymous () {
    kerneltypes = d.getVar('KERNEL_IMAGETYPES') or ""
    if 'fitImage' in kerneltypes.split():
        depends = d.getVar("DEPENDS")
        depends = "%s u-boot-tools-native dtc-native" % depends
        d.setVar("DEPENDS", depends)

        uarch = d.getVar("UBOOT_ARCH")
        if uarch == "arm64":
            replacementtype = "Image"
        elif uarch == "riscv":
            replacementtype = "Image"
        elif uarch == "mips":
            replacementtype = "vmlinuz.bin"
        elif uarch == "x86":
            replacementtype = "bzImage"
        elif uarch == "microblaze":
            replacementtype = "linux.bin"
        else:
            replacementtype = "zImage"

        d.setVar("KERNEL_IMAGETYPE_REPLACEMENT", replacementtype)

        # Override KERNEL_IMAGETYPE_FOR_MAKE variable, which is internal
        # to kernel.bbclass . We have to override it, since we pack zImage
        # (at least for now) into the fitImage .
        typeformake = d.getVar("KERNEL_IMAGETYPE_FOR_MAKE") or ""
        if 'fitImage' in typeformake.split():
            d.setVar('KERNEL_IMAGETYPE_FOR_MAKE', typeformake.replace('fitImage', replacementtype))

        image = d.getVar('INITRAMFS_IMAGE')
        if image:
            d.appendVarFlag('do_assemble_fitimage_initramfs', 'depends', ' ${INITRAMFS_IMAGE}:do_image_complete')

        #check if there are any dtb providers
        providerdtb = d.getVar("PREFERRED_PROVIDER_virtual/dtb")
        if providerdtb:
            d.appendVarFlag('do_assemble_fitimage', 'depends', ' virtual/dtb:do_populate_sysroot')
            d.appendVarFlag('do_assemble_fitimage_initramfs', 'depends', ' virtual/dtb:do_populate_sysroot')
            d.setVar('EXTERNAL_KERNEL_DEVICETREE', "${RECIPE_SYSROOT}/boot/devicetree")

        # Verified boot will sign the fitImage and append the public key to
        # U-Boot dtb. We ensure the U-Boot dtb is deployed before assembling
        # the fitImage:
        if d.getVar('UBOOT_SIGN_ENABLE') == "1" and d.getVar('UBOOT_DTB_BINARY'):
            uboot_pn = d.getVar('PREFERRED_PROVIDER_u-boot') or 'u-boot'
            d.appendVarFlag('do_assemble_fitimage', 'depends', ' %s:do_populate_sysroot' % uboot_pn)
            if d.getVar('INITRAMFS_IMAGE_BUNDLE') == "1":
                d.appendVarFlag('do_assemble_fitimage_initramfs', 'depends', ' %s:do_populate_sysroot' % uboot_pn)
}


# Description string
FIT_DESC ?= "Kernel fitImage for ${DISTRO_NAME}/${PV}/${MACHINE}"

# Sign individual images as well
FIT_SIGN_INDIVIDUAL ?= "0"

#
# Emit the fitImage ITS header
#
# $1 ... .its filename
fitimage_emit_fit_header() {
	cat << EOF >> ${1}
/dts-v1/;

/ {
        description = "${FIT_DESC}";
        #address-cells = <1>;
EOF
}

#
# Emit the fitImage section bits
#
# $1 ... .its filename
# $2 ... Section bit type: imagestart - image section start
#                          confstart  - configuration section start
#                          sectend    - section end
#                          fitend     - fitimage end
#
fitimage_emit_section_maint() {
	case $2 in
	imagestart)
		cat << EOF >> ${1}

        images {
EOF
	;;
	confstart)
		cat << EOF >> ${1}

        configurations {
EOF
	;;
	sectend)
		cat << EOF >> ${1}
	};
EOF
	;;
	fitend)
		cat << EOF >> ${1}
};
EOF
	;;
	esac
}

#
# Emit the fitImage ITS kernel section
#
# $1 ... .its filename
# $2 ... Image counter
# $3 ... Path to kernel image
# $4 ... Compression type
fitimage_emit_section_kernel() {

	kernel_csum="${FIT_HASH_ALG}"
	kernel_sign_algo="${FIT_SIGN_ALG}"
	kernel_sign_keyname="${UBOOT_SIGN_KEYNAME}"

	ENTRYPOINT="${UBOOT_ENTRYPOINT}"
	if [ -n "${UBOOT_ENTRYSYMBOL}" ]; then
		ENTRYPOINT=`${HOST_PREFIX}nm vmlinux | \
			awk '$3=="${UBOOT_ENTRYSYMBOL}" {print "0x"$1;exit}'`
	fi

	cat << EOF >> ${1}
                kernel-${2} {
                        description = "Linux kernel";
                        data = /incbin/("${3}");
                        type = "kernel";
                        arch = "${UBOOT_ARCH}";
                        os = "linux";
                        compression = "${4}";
                        load = <${UBOOT_LOADADDRESS}>;
                        entry = <${ENTRYPOINT}>;
                        hash-1 {
                                algo = "${kernel_csum}";
                        };
                };
EOF

	if [ "${UBOOT_SIGN_ENABLE}" = "1" -a "${FIT_SIGN_INDIVIDUAL}" = "1" -a -n "${kernel_sign_keyname}" ] ; then
		sed -i '$ d' ${1}
		cat << EOF >> ${1}
                        signature-1 {
                                algo = "${kernel_csum},${kernel_sign_algo}";
                                key-name-hint = "${kernel_sign_keyname}";
                        };
                };
EOF
	fi
}

#
# Emit the fitImage ITS DTB section
#
# $1 ... .its filename
# $2 ... Image counter
# $3 ... Path to DTB image
fitimage_emit_section_dtb() {

	dtb_csum="${FIT_HASH_ALG}"
	dtb_sign_algo="${FIT_SIGN_ALG}"
	dtb_sign_keyname="${UBOOT_SIGN_KEYNAME}"

	dtb_loadline=""
	dtb_ext=${DTB##*.}
	if [ "${dtb_ext}" = "dtbo" ]; then
		if [ -n "${UBOOT_DTBO_LOADADDRESS}" ]; then
			dtb_loadline="load = <${UBOOT_DTBO_LOADADDRESS}>;"
		fi
	elif [ -n "${UBOOT_DTB_LOADADDRESS}" ]; then
		dtb_loadline="load = <${UBOOT_DTB_LOADADDRESS}>;"
	fi
	cat << EOF >> ${1}
                fdt-${2} {
                        description = "Flattened Device Tree blob";
                        data = /incbin/("${3}");
                        type = "flat_dt";
                        arch = "${UBOOT_ARCH}";
                        compression = "none";
                        ${dtb_loadline}
                        hash-1 {
                                algo = "${dtb_csum}";
                        };
                };
EOF

	if [ "${UBOOT_SIGN_ENABLE}" = "1" -a "${FIT_SIGN_INDIVIDUAL}" = "1" -a -n "${dtb_sign_keyname}" ] ; then
		sed -i '$ d' ${1}
		cat << EOF >> ${1}
                        signature-1 {
                                algo = "${dtb_csum},${dtb_sign_algo}";
                                key-name-hint = "${dtb_sign_keyname}";
                        };
                };
EOF
	fi
}

#
# Emit the fitImage ITS u-boot script section
#
# $1 ... .its filename
# $2 ... Image counter
# $3 ... Path to boot script image
fitimage_emit_section_boot_script() {

        bootscr_csum="${FIT_HASH_ALG}"
	bootscr_sign_algo="${FIT_SIGN_ALG}"
	bootscr_sign_keyname="${UBOOT_SIGN_KEYNAME}"

        cat << EOF >> ${1}
                bootscr@${2} {
                        description = "U-boot script";
                        data = /incbin/("${3}");
                        type = "script";
                        arch = "${UBOOT_ARCH}";
                        compression = "none";
                        hash@1 {
                                algo = "${bootscr_csum}";
                        };
                };
EOF

	if [ "${UBOOT_SIGN_ENABLE}" = "1" -a "${FIT_SIGN_INDIVIDUAL}" = "1" -a -n "${bootscr_sign_keyname}" ] ; then
		sed -i '$ d' ${1}
		cat << EOF >> ${1}
                        signature@1 {
                                algo = "${bootscr_csum},${bootscr_sign_algo}";
                                key-name-hint = "${bootscr_sign_keyname}";
                        };
                };
EOF
	fi
}

#
# Emit the fitImage ITS setup section
#
# $1 ... .its filename
# $2 ... Image counter
# $3 ... Path to setup image
fitimage_emit_section_setup() {

	setup_csum="${FIT_HASH_ALG}"

	cat << EOF >> ${1}
                setup-${2} {
                        description = "Linux setup.bin";
                        data = /incbin/("${3}");
                        type = "x86_setup";
                        arch = "${UBOOT_ARCH}";
                        os = "linux";
                        compression = "none";
                        load = <0x00090000>;
                        entry = <0x00090000>;
                        hash-1 {
                                algo = "${setup_csum}";
                        };
                };
EOF
}

#
# Emit the fitImage ITS ramdisk section
#
# $1 ... .its filename
# $2 ... Image counter
# $3 ... Path to ramdisk image
fitimage_emit_section_ramdisk() {

	ramdisk_csum="${FIT_HASH_ALG}"
	ramdisk_sign_algo="${FIT_SIGN_ALG}"
	ramdisk_sign_keyname="${UBOOT_SIGN_KEYNAME}"
	ramdisk_loadline=""
	ramdisk_entryline=""

	if [ -n "${UBOOT_RD_LOADADDRESS}" ]; then
		ramdisk_loadline="load = <${UBOOT_RD_LOADADDRESS}>;"
	fi
	if [ -n "${UBOOT_RD_ENTRYPOINT}" ]; then
		ramdisk_entryline="entry = <${UBOOT_RD_ENTRYPOINT}>;"
	fi

	cat << EOF >> ${1}
                ramdisk-${2} {
                        description = "${INITRAMFS_IMAGE}";
                        data = /incbin/("${3}");
                        type = "ramdisk";
                        arch = "${UBOOT_ARCH}";
                        os = "linux";
                        compression = "none";
                        ${ramdisk_loadline}
                        ${ramdisk_entryline}
                        hash-1 {
                                algo = "${ramdisk_csum}";
                        };
                };
EOF

	if [ "${UBOOT_SIGN_ENABLE}" = "1" -a "${FIT_SIGN_INDIVIDUAL}" = "1" -a -n "${ramdisk_sign_keyname}" ] ; then
		sed -i '$ d' ${1}
		cat << EOF >> ${1}
                        signature-1 {
                                algo = "${ramdisk_csum},${ramdisk_sign_algo}";
                                key-name-hint = "${ramdisk_sign_keyname}";
                        };
                };
EOF
	fi
}

#
# Emit the fitImage ITS configuration section
#
# $1 ... .its filename
# $2 ... Linux kernel ID
# $3 ... DTB image name
# $4 ... ramdisk ID
# $5 ... u-boot script ID
# $6 ... config ID
# $7 ... default flag
fitimage_emit_section_config() {

	conf_csum="${FIT_HASH_ALG}"
	conf_sign_algo="${FIT_SIGN_ALG}"
	if [ -n "${UBOOT_SIGN_ENABLE}" ] ; then
		conf_sign_keyname="${UBOOT_SIGN_KEYNAME}"
	fi

	its_file="${1}"
	kernel_id="${2}"
	dtb_image="${3}"
	ramdisk_id="${4}"
	bootscr_id="${5}"
	config_id="${6}"
	default_flag="${7}"

	# Test if we have any DTBs at all
	sep=""
	conf_desc=""
	conf_node="conf-"
	kernel_line=""
	fdt_line=""
	ramdisk_line=""
	bootscr_line=""
	setup_line=""
	default_line=""

	# conf node name is selected based on dtb ID if it is present,
	# otherwise its selected based on kernel ID
	if [ -n "${dtb_image}" ]; then
		conf_node=$conf_node${dtb_image}
	else
		conf_node=$conf_node${kernel_id}
	fi

	if [ -n "${kernel_id}" ]; then
		conf_desc="Linux kernel"
		sep=", "
		kernel_line="kernel = \"kernel-${kernel_id}\";"
	fi

	if [ -n "${dtb_image}" ]; then
		conf_desc="${conf_desc}${sep}FDT blob"
		sep=", "
		fdt_line="fdt = \"fdt-${dtb_image}\";"
	fi

	if [ -n "${ramdisk_id}" ]; then
		conf_desc="${conf_desc}${sep}ramdisk"
		sep=", "
		ramdisk_line="ramdisk = \"ramdisk-${ramdisk_id}\";"
	fi

	if [ -n "${bootscr_id}" ]; then
		conf_desc="${conf_desc}${sep}u-boot script"
		sep=", "
		bootscr_line="bootscr = \"bootscr@${bootscr_id}\";"
	fi

	if [ -n "${config_id}" ]; then
		conf_desc="${conf_desc}${sep}setup"
		setup_line="setup = \"setup-${config_id}\";"
	fi

	if [ "${default_flag}" = "1" ]; then
		# default node is selected based on dtb ID if it is present,
		# otherwise its selected based on kernel ID
		if [ -n "${dtb_image}" ]; then
			default_line="default = \"conf-${dtb_image}\";"
		else
			default_line="default = \"conf-${kernel_id}\";"
		fi
	fi

	cat << EOF >> ${its_file}
                ${default_line}
                $conf_node {
			description = "${default_flag} ${conf_desc}";
			${kernel_line}
			${fdt_line}
			${ramdisk_line}
			${bootscr_line}
			${setup_line}
                        hash-1 {
                                algo = "${conf_csum}";
                        };
EOF

	if [ ! -z "${conf_sign_keyname}" ] ; then

		sign_line="sign-images = "
		sep=""

		if [ -n "${kernel_id}" ]; then
			sign_line="${sign_line}${sep}\"kernel\""
			sep=", "
		fi

		if [ -n "${dtb_image}" ]; then
			sign_line="${sign_line}${sep}\"fdt\""
			sep=", "
		fi

		if [ -n "${ramdisk_id}" ]; then
			sign_line="${sign_line}${sep}\"ramdisk\""
			sep=", "
		fi

		if [ -n "${bootscr_id}" ]; then
			sign_line="${sign_line}${sep}\"bootscr\""
			sep=", "
		fi

		if [ -n "${config_id}" ]; then
			sign_line="${sign_line}${sep}\"setup\""
		fi

		sign_line="${sign_line};"

		cat << EOF >> ${its_file}
                        signature-1 {
                                algo = "${conf_csum},${conf_sign_algo}";
                                key-name-hint = "${conf_sign_keyname}";
				${sign_line}
                        };
EOF
	fi

	cat << EOF >> ${its_file}
                };
EOF
}

#
# Assemble fitImage
#
# $1 ... .its filename
# $2 ... fitImage name
# $3 ... include ramdisk
fitimage_assemble() {
	kernelcount=1
	dtbcount=""
	DTBS=""
	ramdiskcount=${3}
	setupcount=""
	bootscr_id=""
	rm -f ${1} arch/${ARCH}/boot/${2}

	fitimage_emit_fit_header ${1}

	#
	# Step 1: Prepare a kernel image section.
	#
	fitimage_emit_section_maint ${1} imagestart

	uboot_prep_kimage

	if [ "${INITRAMFS_IMAGE_BUNDLE}" = "1" ]; then
		initramfs_bundle_path="arch/"${UBOOT_ARCH}"/boot/"${KERNEL_IMAGETYPE_REPLACEMENT}".initramfs"
		if [ -e "${initramfs_bundle_path}" ]; then

			#
			# Include the kernel/rootfs bundle.
			#

			fitimage_emit_section_kernel ${1} "${kernelcount}" "${initramfs_bundle_path}" "${linux_comp}"
		else
			bbwarn "${initramfs_bundle_path} not found."
		fi
	else
		fitimage_emit_section_kernel ${1} "${kernelcount}" linux.bin "${linux_comp}"
	fi

	#
	# Step 2: Prepare a DTB image section
	#

	if [ -n "${KERNEL_DEVICETREE}" ]; then
		dtbcount=1
		for DTB in ${KERNEL_DEVICETREE}; do
			if echo ${DTB} | grep -q '/dts/'; then
				bbwarn "${DTB} contains the full path to the the dts file, but only the dtb name should be used."
				DTB=`basename ${DTB} | sed 's,\.dts$,.dtb,g'`
			fi

			# Skip ${DTB} if it's also provided in ${EXTERNAL_KERNEL_DEVICETREE}
			if [ -n "${EXTERNAL_KERNEL_DEVICETREE}" ] && [ -s ${EXTERNAL_KERNEL_DEVICETREE}/${DTB} ]; then
				continue
			fi

			DTB_PATH="arch/${ARCH}/boot/dts/${DTB}"
			if [ ! -e "${DTB_PATH}" ]; then
				DTB_PATH="arch/${ARCH}/boot/${DTB}"
			fi

			DTB=$(echo "${DTB}" | tr '/' '_')
			DTBS="${DTBS} ${DTB}"
			fitimage_emit_section_dtb ${1} ${DTB} ${DTB_PATH}
		done
	fi

	if [ -n "${EXTERNAL_KERNEL_DEVICETREE}" ]; then
		dtbcount=1
		for DTB in $(find "${EXTERNAL_KERNEL_DEVICETREE}" \( -name '*.dtb' -o -name '*.dtbo' \) -printf '%P\n' | sort); do
			DTB=$(echo "${DTB}" | tr '/' '_')
			DTBS="${DTBS} ${DTB}"
			fitimage_emit_section_dtb ${1} ${DTB} "${EXTERNAL_KERNEL_DEVICETREE}/${DTB}"
		done
	fi

	#
	# Step 3: Prepare a u-boot script section
	#

	if [ -n "${UBOOT_ENV}" ] && [ -d "${STAGING_DIR_HOST}/boot" ]; then
		if [ -e "${STAGING_DIR_HOST}/boot/${UBOOT_ENV_BINARY}" ]; then
			cp ${STAGING_DIR_HOST}/boot/${UBOOT_ENV_BINARY} ${B}
			bootscr_id="${UBOOT_ENV_BINARY}"
			fitimage_emit_section_boot_script ${1} "${bootscr_id}" ${UBOOT_ENV_BINARY}
		else
			bbwarn "${STAGING_DIR_HOST}/boot/${UBOOT_ENV_BINARY} not found."
		fi
	fi

	#
	# Step 4: Prepare a setup section. (For x86)
	#
	if [ -e arch/${ARCH}/boot/setup.bin ]; then
		setupcount=1
		fitimage_emit_section_setup ${1} "${setupcount}" arch/${ARCH}/boot/setup.bin
	fi

	#
	# Step 5: Prepare a ramdisk section.
	#
	if [ "x${ramdiskcount}" = "x1" ] && [ "${INITRAMFS_IMAGE_BUNDLE}" != "1" ]; then
		# Find and use the first initramfs image archive type we find
		for img in cpio.lz4 cpio.lzo cpio.lzma cpio.xz cpio.gz ext2.gz cpio; do
			initramfs_path="${DEPLOY_DIR_IMAGE}/${INITRAMFS_IMAGE_NAME}.${img}"
			echo "Using $initramfs_path"
			if [ -e "${initramfs_path}" ]; then
				fitimage_emit_section_ramdisk ${1} "${ramdiskcount}" "${initramfs_path}"
				break
			fi
		done
	fi

	fitimage_emit_section_maint ${1} sectend

	# Force the first Kernel and DTB in the default config
	kernelcount=1
	if [ -n "${dtbcount}" ]; then
		dtbcount=1
	fi

	#
	# Step 6: Prepare a configurations section
	#
	fitimage_emit_section_maint ${1} confstart

	# kernel-fitimage.bbclass currently only supports a single kernel (no less or
	# more) to be added to the FIT image along with 0 or more device trees and
	# 0 or 1 ramdisk.
        # It is also possible to include an initramfs bundle (kernel and rootfs in one binary)
        # When the initramfs bundle is used ramdisk is disabled.
	# If a device tree is to be part of the FIT image, then select
	# the default configuration to be used is based on the dtbcount. If there is
	# no dtb present than select the default configuation to be based on
	# the kernelcount.
	if [ -n "${DTBS}" ]; then
		i=1
		for DTB in ${DTBS}; do
			dtb_ext=${DTB##*.}
			if [ "${dtb_ext}" = "dtbo" ]; then
				fitimage_emit_section_config ${1} "" "${DTB}" "" "${bootscr_id}" "" "`expr ${i} = ${dtbcount}`"
			else
				fitimage_emit_section_config ${1} "${kernelcount}" "${DTB}" "${ramdiskcount}" "${bootscr_id}" "${setupcount}" "`expr ${i} = ${dtbcount}`"
			fi
			i=`expr ${i} + 1`
		done
	else
		defaultconfigcount=1
		fitimage_emit_section_config ${1} "${kernelcount}" "" "${ramdiskcount}" "${bootscr_id}"  "${setupcount}" "${defaultconfigcount}"
	fi

	fitimage_emit_section_maint ${1} sectend

	fitimage_emit_section_maint ${1} fitend

	#
	# Step 7: Assemble the image
	#
	${UBOOT_MKIMAGE} \
		${@'-D "${UBOOT_MKIMAGE_DTCOPTS}"' if len('${UBOOT_MKIMAGE_DTCOPTS}') else ''} \
		-f ${1} \
		arch/${ARCH}/boot/${2}

	#
	# Step 8: Sign the image and add public key to U-Boot dtb
	#
	if [ "x${UBOOT_SIGN_ENABLE}" = "x1" ] ; then
		add_key_to_u_boot=""
		if [ -n "${UBOOT_DTB_BINARY}" ]; then
			# The u-boot.dtb is a symlink to UBOOT_DTB_IMAGE, so we need copy
			# both of them, and don't dereference the symlink.
			cp -P ${STAGING_DATADIR}/u-boot*.dtb ${B}
			add_key_to_u_boot="-K ${B}/${UBOOT_DTB_BINARY}"
		fi
		${UBOOT_MKIMAGE_SIGN} \
			${@'-D "${UBOOT_MKIMAGE_DTCOPTS}"' if len('${UBOOT_MKIMAGE_DTCOPTS}') else ''} \
			-F -k "${UBOOT_SIGN_KEYDIR}" \
			$add_key_to_u_boot \
			-r arch/${ARCH}/boot/${2} \
			${UBOOT_MKIMAGE_SIGN_ARGS}
	fi
}

do_assemble_fitimage() {
	if echo ${KERNEL_IMAGETYPES} | grep -wq "fitImage"; then
		cd ${B}
		fitimage_assemble fit-image.its fitImage
	fi
}

addtask assemble_fitimage before do_install after do_compile

do_assemble_fitimage_initramfs() {
	if echo ${KERNEL_IMAGETYPES} | grep -wq "fitImage" && \
		test -n "${INITRAMFS_IMAGE}" ; then
		cd ${B}
		if [ "${INITRAMFS_IMAGE_BUNDLE}" = "1" ]; then
			fitimage_assemble fit-image-${INITRAMFS_IMAGE}.its fitImage ""
		else
			fitimage_assemble fit-image-${INITRAMFS_IMAGE}.its fitImage-${INITRAMFS_IMAGE} 1
		fi
	fi
}

addtask assemble_fitimage_initramfs before do_deploy after do_bundle_initramfs

addtask generate_rsa_keys before do_assemble_fitimage after do_compile

kernel_do_deploy[vardepsexclude] = "DATETIME"
kernel_do_deploy_append() {
	# Update deploy directory
	if echo ${KERNEL_IMAGETYPES} | grep -wq "fitImage"; then

		if [ "${INITRAMFS_IMAGE_BUNDLE}" != "1" ]; then
			echo "Copying fit-image.its source file..."
			install -m 0644 ${B}/fit-image.its "$deployDir/fitImage-its-${KERNEL_FIT_NAME}.its"
			ln -snf fitImage-its-${KERNEL_FIT_NAME}.its "$deployDir/fitImage-its-${KERNEL_FIT_LINK_NAME}"

			echo "Copying linux.bin file..."
			install -m 0644 ${B}/linux.bin $deployDir/fitImage-linux.bin-${KERNEL_FIT_NAME}.bin
			ln -snf fitImage-linux.bin-${KERNEL_FIT_NAME}.bin "$deployDir/fitImage-linux.bin-${KERNEL_FIT_LINK_NAME}"
		fi

		if [ -n "${INITRAMFS_IMAGE}" ]; then
			echo "Copying fit-image-${INITRAMFS_IMAGE}.its source file..."
			install -m 0644 ${B}/fit-image-${INITRAMFS_IMAGE}.its "$deployDir/fitImage-its-${INITRAMFS_IMAGE_NAME}-${KERNEL_FIT_NAME}.its"
			ln -snf fitImage-its-${INITRAMFS_IMAGE_NAME}-${KERNEL_FIT_NAME}.its "$deployDir/fitImage-its-${INITRAMFS_IMAGE_NAME}-${KERNEL_FIT_LINK_NAME}"

			if [ "${INITRAMFS_IMAGE_BUNDLE}" != "1" ]; then
				echo "Copying fitImage-${INITRAMFS_IMAGE} file..."
				install -m 0644 ${B}/arch/${ARCH}/boot/fitImage-${INITRAMFS_IMAGE} "$deployDir/fitImage-${INITRAMFS_IMAGE_NAME}-${KERNEL_FIT_NAME}.bin"
				ln -snf fitImage-${INITRAMFS_IMAGE_NAME}-${KERNEL_FIT_NAME}.bin "$deployDir/fitImage-${INITRAMFS_IMAGE_NAME}-${KERNEL_FIT_LINK_NAME}"
			fi
		fi
	fi
	if [ "${UBOOT_SIGN_ENABLE}" = "1" -o "${UBOOT_FITIMAGE_ENABLE}" = "1" ] && \
	   [ -n "${UBOOT_DTB_BINARY}" ] ; then
		# UBOOT_DTB_IMAGE is a realfile, but we can't use
		# ${UBOOT_DTB_IMAGE} since it contains ${PV} which is aimed
		# for u-boot, but we are in kernel env now.
		install -m 0644 ${B}/u-boot-${MACHINE}*.dtb "$deployDir/"
	fi
	if [ "${UBOOT_FITIMAGE_ENABLE}" = "1" -a -n "${UBOOT_BINARY}" -a -n "${SPL_DTB_BINARY}" ] ; then
		# If we're also creating and/or signing the uboot fit, now we need to
		# deploy it, it's its file, as well as u-boot-spl.dtb
		install -m 0644 ${B}/u-boot-spl-${MACHINE}*.dtb "$deployDir/"
		echo "Copying u-boot-fitImage file..."
		install -m 0644 ${B}/u-boot-fitImage-* "$deployDir/"
		echo "Copying u-boot-its file..."
		install -m 0644 ${B}/u-boot-its-* "$deployDir/"
	fi
}

# The function below performs the following in case of initramfs bundles:
# - Removes do_assemble_fitimage. FIT generation is done through
#   do_assemble_fitimage_initramfs. do_assemble_fitimage is not needed
#   and should not be part of the tasks to be executed.
# - Since do_generate_rsa_keys is inserted by default
#   between do_compile and do_assemble_fitimage, this is
#   not suitable in case of initramfs bundles.  do_generate_rsa_keys
#   should be between do_bundle_initramfs and do_assemble_fitimage_initramfs.
python () {
    if d.getVar('INITRAMFS_IMAGE_BUNDLE') == "1":
        bb.build.deltask('do_assemble_fitimage', d)
        bb.build.deltask('generate_rsa_keys', d)
        bb.build.addtask('generate_rsa_keys', 'do_assemble_fitimage_initramfs', 'do_bundle_initramfs', d)
}
