From 809330ab8450261e05919b472783bf15e4b000f7 Mon Sep 17 00:00:00 2001
From: Richard Earnshaw <rearnsha@arm.com>
Date: Tue, 6 Jul 2021 15:10:18 +0100
Subject: [PATCH] arm: Add tests for VLLDM mitigation [PR102035]

New tests for the erratum mitigation.

gcc/testsuite:
	PR target/102035
	* gcc.target/arm/cmse/mainline/8_1m/soft/cmse-13a.c: New test.
	* gcc.target/arm/cmse/mainline/8_1m/soft/cmse-7a.c: Likewise.
	* gcc.target/arm/cmse/mainline/8_1m/soft/cmse-8a.c: Likewise.
	* gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-7a.c: Likewise.
	* gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-8a.c: Likewise.
	* gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-13a.c: Likewise.
	* gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-7a.c: Likewise.
	* gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-8a.c: Likewise.

CVE: CVE-2021-35465
Upstream-Status: Backport[https://gcc.gnu.org/git/gitweb.cgi?p=gcc.git;h=809330ab8450261e05919b472783bf15e4b000f7]
Signed-off-by: Pgowda <pgowda.cve@gmail.com>

---
 .../arm/cmse/mainline/8_1m/soft/cmse-13a.c    | 31 +++++++++++++++++++
 .../arm/cmse/mainline/8_1m/soft/cmse-7a.c     | 28 +++++++++++++++++
 .../arm/cmse/mainline/8_1m/soft/cmse-8a.c     | 30 ++++++++++++++++++
 .../cmse/mainline/8_1m/softfp-sp/cmse-7a.c    | 27 ++++++++++++++++
 .../cmse/mainline/8_1m/softfp-sp/cmse-8a.c    | 29 +++++++++++++++++
 .../arm/cmse/mainline/8_1m/softfp/cmse-13a.c  | 30 ++++++++++++++++++
 .../arm/cmse/mainline/8_1m/softfp/cmse-7a.c   | 27 ++++++++++++++++
 .../arm/cmse/mainline/8_1m/softfp/cmse-8a.c   | 29 +++++++++++++++++
 8 files changed, 231 insertions(+)
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-13a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-7a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-8a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-7a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-8a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-13a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-7a.c
 create mode 100644 gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-8a.c

diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-13a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-13a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-13a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-13a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,31 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=soft -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=soft" } } */
+
+#include "../../../cmse-13.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[1,4-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[1,4-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler-not "mov\tr0, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr2, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr3, r4" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r1, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[1,4-9\]|r10|fp|ip), ){9}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[1,4-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler-not "vmov" } } */
+/* { dg-final { scan-assembler-not "vmsr" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-7a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-7a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-7a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-7a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,28 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=soft -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=soft" } } */
+
+#include "../../../cmse-7.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[0-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[0-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r0, )?(r1, )?(r2, )?(r3, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[0-9\]|r10|fp|ip), ){12}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[0-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler-not "vmov" } } */
+/* { dg-final { scan-assembler-not "vmsr" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-8a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-8a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-8a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/soft/cmse-8a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,30 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=soft -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=soft" } } */
+
+#include "../../../cmse-8.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[2-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[2-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler-not "mov\tr0, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr1, r4" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r2, )?(r3, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[2-9\]|r10|fp|ip), ){10}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[2-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler-not "vmov" } } */
+/* { dg-final { scan-assembler-not "vmsr" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-13a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-13a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-13a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-13a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,30 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=softfp -mfpu=fpv5-d16 -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=softfp" } } */
+/* { dg-skip-if "Skip these if testing single precision" {*-*-*} {"-mfpu=*-sp-*"} {""} } */
+
+#include "../../../cmse-13.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[1,4-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[1,4-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler-not "mov\tr0, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr2, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr3, r4" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r1, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[1,4-9\]|r10|fp|ip), ){9}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[1,4-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-7a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-7a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-7a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-7a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,27 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=softfp -mfpu=fpv5-d16 -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=softfp" } } */
+/* { dg-skip-if "Skip these if testing single precision" {*-*-*} {"-mfpu=*-sp-*"} {""} } */
+
+#include "../../../cmse-7.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[0-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[0-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r0, )?(r1, )?(r2, )?(r3, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[0-9\]|r10|fp|ip), ){12}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[0-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-8a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-8a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-8a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp/cmse-8a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,29 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=softfp -mfpu=fpv5-d16 -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=softfp" } } */
+/* { dg-skip-if "Skip these if testing single precision" {*-*-*} {"-mfpu=*-sp-*"} {""} } */
+
+#include "../../../cmse-8.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[2-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[2-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler-not "mov\tr0, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr1, r4" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r2, )?(r3, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[2-9\]|r10|fp|ip), ){10}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[2-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-7a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-7a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-7a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-7a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,27 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=softfp -mfpu=fpv5-sp-d16 -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=softfp" } } */
+/* { dg-skip-if "Skip these if testing double precision" {*-*-*} {"-mfpu=fpv[4-5]-d16"} {""} } */
+
+#include "../../../cmse-7.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[0-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[0-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r0, )?(r1, )?(r2, )?(r3, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[0-9\]|r10|fp|ip), ){12}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[0-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
diff --git a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-8a.c b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-8a.c
--- a/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-8a.c	1969-12-31 16:00:00.000000000 -0800
+++ b/gcc/testsuite/gcc.target/arm/cmse/mainline/8_1m/softfp-sp/cmse-8a.c	2021-11-15 02:30:37.210637445 -0800
@@ -0,0 +1,29 @@
+/* { dg-do compile } */
+/* { dg-options "-mcmse -mfloat-abi=softfp -mfpu=fpv5-sp-d16 -mfix-cmse-cve-2021-35465" }  */
+/* { dg-skip-if "Incompatible float ABI" { *-*-* } { "-mfloat-abi=*" } { "-mfloat-abi=softfp" } } */
+/* { dg-skip-if "Skip these if testing double precision" {*-*-*} {"-mfpu=fpv[4-5]-d16"} {""} } */
+
+#include "../../../cmse-8.x"
+
+/* Checks for saving and clearing prior to function call.  */
+/* Shift on the same register as blxns.  */
+/* { dg-final { scan-assembler "lsrs\t(r\[2-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler "lsls\t(r\[2-9\]|r10|fp|ip), \\1, #1.*blxns\t\\1" } } */
+/* { dg-final { scan-assembler-not "mov\tr0, r4" } } */
+/* { dg-final { scan-assembler-not "mov\tr1, r4" } } */
+/* { dg-final { scan-assembler "push\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+/* { dg-final { scan-assembler "vlstm\tsp" } } */
+/* Check the right registers are cleared and none appears twice.  */
+/* { dg-final { scan-assembler "clrm\t\{(r2, )?(r3, )?(r4, )?(r5, )?(r6, )?(r7, )?(r8, )?(r9, )?(r10, )?(fp, )?(ip, )?APSR\}" } } */
+/* Check that the right number of registers is cleared and thus only one
+   register is missing.  */
+/* { dg-final { scan-assembler "clrm\t\{((r\[2-9\]|r10|fp|ip), ){10}APSR\}" } } */
+/* Check that no cleared register is used for blxns.  */
+/* { dg-final { scan-assembler-not "clrm\t\{\[^\}\]\+(r\[2-9\]|r10|fp|ip),\[^\}\]\+\}.*blxns\t\\1" } } */
+/* Check for v8.1-m variant of erratum work-around.  */
+/* { dg-final { scan-assembler "vscclrm\t\{vpr\}" } } */
+/* { dg-final { scan-assembler "vlldm\tsp" } } */
+/* { dg-final { scan-assembler "pop\t\{r4, r5, r6, r7, r8, r9, r10, fp\}" } } */
+
+/* Now we check that we use the correct intrinsic to call.  */
+/* { dg-final { scan-assembler "blxns" } } */
