From 30461cf8dba3d3adb15a125e4da48800eb2b9b8f Mon Sep 17 00:00:00 2001
From: Richard Earnshaw <rearnsha@arm.com>
Date: Fri, 18 Jun 2021 17:18:37 +0100
Subject: [PATCH] arm: fix vlldm erratum for Armv8.1-m [PR102035]

For Armv8.1-m we generate code that emits VLLDM directly and do not
rely on support code in the library, so emit the mitigation directly
as well, when required.  In this case, we can use the compiler options
to determine when to apply the fix and when it is safe to omit it.

gcc:
	PR target/102035
	* config/arm/arm.md (attribute arch): Add fix_vlldm.
	(arch_enabled): Use it.
	* config/arm/vfp.md (lazy_store_multiple_insn): Add alternative to
	use when erratum mitigation is needed.

CVE: CVE-2021-35465
Upstream-Status: Backport[https://gcc.gnu.org/git/gitweb.cgi?p=gcc.git;h=30461cf8dba3d3adb15a125e4da48800eb2b9b8f]
Signed-off-by: Pgowda <pgowda.cve@gmail.com>

---
 gcc/config/arm/arm.md | 11 +++++++++--
 gcc/config/arm/vfp.md | 10 +++++++---
 2 files changed, 16 insertions(+), 5 deletions(-)

diff -upr a/gcc/config/arm/arm.md b/gcc/config/arm/arm.md
--- a/gcc/config/arm/arm.md	2020-07-22 23:35:17.344384552 -0700
+++ b/gcc/config/arm/arm.md	2021-11-11 20:33:58.431543947 -0800
@@ -132,9 +132,12 @@
 ; TARGET_32BIT, "t1" or "t2" to specify a specific Thumb mode.  "v6"
 ; for ARM or Thumb-2 with arm_arch6, and nov6 for ARM without
 ; arm_arch6.  "v6t2" for Thumb-2 with arm_arch6 and "v8mb" for ARMv8-M
-; Baseline.  This attribute is used to compute attribute "enabled",
+; Baseline.  "fix_vlldm" is for fixing the v8-m/v8.1-m VLLDM erratum.
+; This attribute is used to compute attribute "enabled",
 ; use type "any" to enable an alternative in all cases.
-(define_attr "arch" "any,a,t,32,t1,t2,v6,nov6,v6t2,v8mb,iwmmxt,iwmmxt2,armv6_or_vfpv3,neon,mve"
+(define_attr "arch" "any, a, t, 32, t1, t2, v6,nov6, v6t2, \
+		     v8mb, fix_vlldm, iwmmxt, iwmmxt2, armv6_or_vfpv3, \
+		     neon, mve"
   (const_string "any"))
 
 (define_attr "arch_enabled" "no,yes"
@@ -177,6 +180,10 @@
 	      (match_test "TARGET_THUMB1 && arm_arch8"))
 	 (const_string "yes")
 
+	 (and (eq_attr "arch" "fix_vlldm")
+	      (match_test "fix_vlldm"))
+	 (const_string "yes")
+
 	 (and (eq_attr "arch" "iwmmxt2")
 	      (match_test "TARGET_REALLY_IWMMXT2"))
 	 (const_string "yes")
diff -upr a/gcc/config/arm/vfp.md b/gcc/config/arm/vfp.md
--- a/gcc/config/arm/vfp.md	2020-07-22 23:35:17.356384684 -0700
+++ b/gcc/config/arm/vfp.md	2021-11-11 20:33:58.431543947 -0800
@@ -1703,12 +1703,15 @@
    (set_attr "type" "mov_reg")]
 )
 
+;; Both this and the next instruction are treated by GCC in the same
+;; way as a blockage pattern.  That's perhaps stronger than it needs
+;; to be, but we do not want accesses to the VFP register bank to be
+;; moved across either instruction.
+
 (define_insn "lazy_store_multiple_insn"
-  [(set (match_operand:SI 0 "s_register_operand" "+&rk")
-	(post_dec:SI (match_dup 0)))
-   (unspec_volatile [(const_int 0)
-		     (mem:SI (post_dec:SI (match_dup 0)))]
-		    VUNSPEC_VLSTM)]
+  [(unspec_volatile
+    [(mem:BLK (match_operand:SI 0 "s_register_operand" "rk"))]
+    VUNSPEC_VLSTM)]
   "use_cmse && reload_completed"
   "vlstm%?\\t%0"
   [(set_attr "predicable" "yes")
@@ -1716,14 +1719,16 @@
 )
 
 (define_insn "lazy_load_multiple_insn"
-  [(set (match_operand:SI 0 "s_register_operand" "+&rk")
-	(post_inc:SI (match_dup 0)))
-   (unspec_volatile:SI [(const_int 0)
-			(mem:SI (match_dup 0))]
-		       VUNSPEC_VLLDM)]
+  [(unspec_volatile
+    [(mem:BLK (match_operand:SI 0 "s_register_operand" "rk,rk"))]
+    VUNSPEC_VLLDM)]
   "use_cmse && reload_completed"
-  "vlldm%?\\t%0"
-  [(set_attr "predicable" "yes")
+  "@
+   vscclrm\\t{vpr}\;vlldm\\t%0
+   vlldm\\t%0"
+  [(set_attr "arch" "fix_vlldm,*")
+   (set_attr "predicable" "no")
+   (set_attr "length" "8,4")
    (set_attr "type" "load_4")]
 )
 
