From afa36390394a6e0cceba03b52b59b6d41710608c Mon Sep 17 00:00:00 2001
From: Cyril Hrubis <metan@ucw.cz>
Date: Fri, 16 May 2025 17:57:10 +0200
Subject: [PATCH] ping: Fix moving average rtt calculation

The rts->rtt counts an exponential weight moving average in a fixed
point, that means that even if we limit the triptime to fit into a 32bit
number the average will overflow because because fixed point needs eight
more bits.

We also have to limit the triptime to 32bit number because otherwise the
moving average may stil overflow if we manage to produce a large enough
triptime.

Fixes: CVE-2025-48964
Fixes: https://bugzilla.suse.com/show_bug.cgi?id=1243772
Closes: https://github.com/iputils/iputils-ghsa-25fr-jw29-74f9/pull/1
Reported-by: Mohamed Maatallah <hotelsmaatallahrecemail@gmail.com>
Reviewed-by: Petr Vorel <pvorel@suse.cz>
Tested-by: Petr Vorel <pvorel@suse.cz>
Reviewed-by: Michal Kubecek <mkubecek@suse.cz>
Reviewed-by: Mohamed Maatallah <hotelsmaatallahrecemail@gmail.com>
Signed-off-by: Cyril Hrubis <metan@ucw.cz>

CVE: CVE-2025-48964
Upstream-Status: Backport [https://github.com/iputils/iputils/commit/afa36390394a6e0cceba03b52b59b6d41710608c]
Signed-off-by: Peter Marko <peter.marko@siemens.com>
---
 iputils_common.h   | 2 +-
 ping/ping.h        | 2 +-
 ping/ping_common.c | 8 ++++----
 3 files changed, 6 insertions(+), 6 deletions(-)

diff --git a/iputils_common.h b/iputils_common.h
index 829a749..1296905 100644
--- a/iputils_common.h
+++ b/iputils_common.h
@@ -11,7 +11,7 @@
 					 __typeof__(&arr[0]))])) * 0)
 
 /* 1000001 = 1000000 tv_sec + 1 tv_usec */
-#define TV_SEC_MAX_VAL (LONG_MAX/1000001)
+#define TV_SEC_MAX_VAL (INT32_MAX/1000001)
 
 #ifdef __GNUC__
 # define iputils_attribute_format(t, n, m) __attribute__((__format__ (t, n, m)))
diff --git a/ping/ping.h b/ping/ping.h
index 4dce538..bc1fab2 100644
--- a/ping/ping.h
+++ b/ping/ping.h
@@ -191,7 +191,7 @@ struct ping_rts {
 	long tmax;			/* maximum round trip time */
 	double tsum;			/* sum of all times, for doing average */
 	double tsum2;
-	int rtt;
+	uint64_t rtt;                   /* Exponential weight moving average calculated in fixed point */
 	int rtt_addend;
 	uint16_t acked;
 	int pipesize;
diff --git a/ping/ping_common.c b/ping/ping_common.c
index 2a3e556..fad5228 100644
--- a/ping/ping_common.c
+++ b/ping/ping_common.c
@@ -282,7 +282,7 @@ int __schedule_exit(int next)
 
 static inline void update_interval(struct ping_rts *rts)
 {
-	int est = rts->rtt ? rts->rtt / 8 : rts->interval * 1000;
+	int est = rts->rtt ? (int)(rts->rtt / 8) : rts->interval * 1000;
 
 	rts->interval = (est + rts->rtt_addend + 500) / 1000;
 	if (rts->uid && rts->interval < MIN_USER_INTERVAL_MS)
@@ -778,7 +778,7 @@ restamp:
 			if (triptime > rts->tmax)
 				rts->tmax = triptime;
 			if (!rts->rtt)
-				rts->rtt = triptime * 8;
+				rts->rtt = ((uint64_t)triptime) * 8;
 			else
 				rts->rtt += triptime - rts->rtt / 8;
 			if (rts->opt_adaptive)
@@ -948,7 +948,7 @@ int finish(struct ping_rts *rts)
 		int ipg = (1000000 * (long long)tv.tv_sec + tv.tv_nsec / 1000) / (rts->ntransmitted - 1);
 
 		printf(_("%sipg/ewma %d.%03d/%d.%03d ms"),
-		       comma, ipg / 1000, ipg % 1000, rts->rtt / 8000, (rts->rtt / 8) % 1000);
+		       comma, ipg / 1000, ipg % 1000, (int)(rts->rtt / 8000), (int)((rts->rtt / 8) % 1000));
 	}
 	putchar('\n');
 	return (!rts->nreceived || (rts->deadline && rts->nreceived < rts->npackets));
@@ -973,7 +973,7 @@ void status(struct ping_rts *rts)
 		fprintf(stderr, _(", min/avg/ewma/max = %ld.%03ld/%lu.%03ld/%d.%03d/%ld.%03ld ms"),
 			(long)rts->tmin / 1000, (long)rts->tmin % 1000,
 			tavg / 1000, tavg % 1000,
-			rts->rtt / 8000, (rts->rtt / 8) % 1000, (long)rts->tmax / 1000, (long)rts->tmax % 1000);
+			(int)(rts->rtt / 8000), (int)((rts->rtt / 8) % 1000), (long)rts->tmax / 1000, (long)rts->tmax % 1000);
 	}
 	fprintf(stderr, "\n");
 }
