From 64b38675c728354e4015e4bec3d975cd4cb8a981 Mon Sep 17 00:00:00 2001
From: Alexander Bulekov <alxndr@bu.edu>
Date: Fri, 26 Feb 2021 13:47:53 -0500
Subject: [PATCH 07/10] rtl8139: switch to use qemu_receive_packet() for
 loopback
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This patch switches to use qemu_receive_packet() which can detect
reentrancy and return early.

This is intended to address CVE-2021-3416.

Cc: Prasad J Pandit <ppandit@redhat.com>
Cc: qemu-stable@nongnu.org
Buglink: https://bugs.launchpad.net/qemu/+bug/1910826
Reviewed-by: Philippe Mathieu-Daudé <philmd@redhat.com
Signed-off-by: Alexander Bulekov <alxndr@bu.edu>
Signed-off-by: Jason Wang <jasowang@redhat.com>

Upstream-Status: Backport [5311fb805a4403bba024e83886fa0e7572265de4]
CVE: CVE-2021-3416

Signed-off-by: Sakib Sajal <sakib.sajal@windriver.com>
---
 hw/net/rtl8139.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/hw/net/rtl8139.c b/hw/net/rtl8139.c
index ba5ace1ab..d2dd03e6a 100644
--- a/hw/net/rtl8139.c
+++ b/hw/net/rtl8139.c
@@ -1795,7 +1795,7 @@ static void rtl8139_transfer_frame(RTL8139State *s, uint8_t *buf, int size,
         }
 
         DPRINTF("+++ transmit loopback mode\n");
-        rtl8139_do_receive(qemu_get_queue(s->nic), buf, size, do_interrupt);
+        qemu_receive_packet(qemu_get_queue(s->nic), buf, size);
 
         if (iov) {
             g_free(buf2);
-- 
2.29.2

